31030-11 Three Thread Interlock Chainstitch Collar Binding Machine
Main Specification & Applications
Model

Needle

Thread

Stitch Length (mm)

Needle gauge (mm)

Differential Rate

Foot Lift (mm)

Needle Type (Gk16)

Hem Width
(mm)

Speed (S. P. M)
Gk31030-11

1.8-3.3

3.3(6)

0.8-1.2

6

70

54x20

4000
Model

Applications
GK31030-11

Available to perform cover stitching ,  Collar binding &  hemming on Garment .   Knitted underwear,  etc.
31030 -11 Other General Spare Parts
	No.
	Ref. No.
	Description
	QT.
	No.
	Ref. No.
	Description
	QT.

	1
	SP085A
	Trade mark plate
	1
	6
	11A1 -009D
	Rollar plate assy.
	1

	2
	107T6-001A
	Presser foot assy.
	1
	7
	12A1 -001
	Front Cover plate sewing desk
	1

	3
	107T4 - 002
	Feed dog
	1
	8
	12A1 -003A
	Binder
	1

	4
	107T4 - 001
	Needle plate
	1
	9
	118T1 -001A
	Binder plug
	1

	5
	107T4-003
	Differential feed dog
	1
	
	
	
	


