
MODEL :  HARMONY SM/PSA 2101

DESCRIPTION

HARMONY SM/PSA 2101 is a foldable ironing table with a built–in steam boiler and manufactured for both professional and domestic use. It has a mechanism to prevent undesirable wetness caused by moisture built-up during an intensive or prolonged ironing operation, condensing and converting to water droplets. The fan sucks and exhausts the vapor before it condenses, and the heating resistance located underneath the ironing board keeps the ironing warm and therefore dries the wetness at once if any.

Main sections and the shape of HARMONY SM/PSA 2101 is shown below.

.

 Switches, Knob and Indicators on the Control Panel  

The control panel is situated on the built-in steam boiler, wherein it is located at the rear of the table, contains control switches and warning lights.  

Switches and lights on the control panel and their functions are as shown below.



















                                       Control Panel.

(1) on – off Switch for Steam Boiler ; It provides to work steam boiler resistance.

(2) on – off Switch for Iron; It provides to work iron resistance.

(3) Temperature Setting Knob: This is a temperature setting knob for controlling the temperature of the ironing surface. When the knob is set to a certain value, the ironing surface temperature will be maintained at a temperature as adjusted by the thermostat and the resistance will heat up as controlled by the thermostat. At OFF position, the resistance is disengaged. Depending on the operating conditions, temperature is not evenly distributed on the ironing surface and is expressed as an average value. The setting and installation is such that the cloth over the ironing surface will not burn at the highest value of temperature setting. 

(4) Resistance Engaged Signal: This warning light will go on as long as the resistance beneath the ironing surface is active.

(5) Manometer: It indicates steam pressure in boiler. 
(6) Steam Ready Signal: “Steam” warning lamp is lit when steam is ready.

(7) No Water Signal: “No water” warning lamp lights up when water runs out.

(8) Fan Pedal: It operates the suction fan. 

TECHNICAL PROPERTIES

	IRONING BOARD UNIT                                         
	IRON / STEAM BOILER UNIT

	Supply
	:
	                                         220/230 V, 50Hz 

	Resistance Power
	:
	600 Watt @ 220 V
	Boiler Resistance
	1000 Watt@ 220 V

	Fan Motor Power
	:
	70   Watt 
	Iron Resistance
	800  Watt@ 220 V

	Fan Suction Capacity
	:
	~200 m3/hours
	Water Capacity
	1 Litre

	Ironing Pad Size
	:
	120 x 39 cm
	Min. Ironing Period
	~ 2 Hours

	Height Adjustment Range
	:
	79-88-95 cm 3 levels
	Steam Pressure
	min. 2 – max. 3 Bar

	Folded Dimensions
	:
	~ 27 x 40 x 153 cm

	Weight
	:
	                                                  ~ 27 kg 


4 Levels Safety System

Device has a 4 levels safety system.

1. A pressure switch in appliance that prevents the boiler overpressure.

2. A bimetal disc thermostat that prevents over-heating.

3. A safety fuse that is activated in the event of failure in bimetal thermostat operation. (In such cases safety fuse cuts the electric power of the boiler and No Water (7) lamp is lit constantly. In this case take your device to the nearest Silter authorized  service.)

4. In the event that above-mentioned safety system fails all together, a mechanical safety valve releases the steam in the boiler automatically.

SAFETY WARNINGS

· Device operates on 220-240V electricity.

· Strictly operate through a grounded socket.

· Do not operate with a damaged electric, pedal cable power cord or steam hose; contact the authorized service for the replacement of damaged parts.

· Avoid touching metal parts of the ironing surface; they may be hot.

· Due to the high temperature of the soleplate of the iron, avoid any kind of the physical contact. You should also be careful while touching the silicone ironing rest, which is used while ironing as per our advice, due to possibility of reaching high temperature after some period. 

· Avoid inserting foreign materials through fan propellers.

· Especially when operating, do not let children come closer to the appliance.

· At times when the appliance is not in use, unplug it for safety reasons. 

· The appliance possesses the specialty of releasing intense and continual steam at high temperature. Straight steam release to skin at close range should be avoided as a precaution.

· Attention: Do not open the valve, that is under the water tank, while operating the appliance!

· Attention: Do not open the cap of the water tank while operating the appliance!

· Before emptying water tank, turn off switch for steam boiler (1) and unplug the device from electric outlet and be sure that the pressure is zero bar on the manometer (5). 

· Before emptying water, place an empty vessel under the water tank.

· Do not excessively tighten the cap of the water tank after filling the water. In case of any damage from such strain, contact the Authorized Silter Service for the replacement of the cap.

· Do not leave the device in operative state if no water (7) lamp is lit during operation.

· For your safety do not open the lid before device pressure falls to zero. For refilling, observe the instructions provided in following pages of this user guide.

ASSEMBLY OF THE APPLIANCE 

               Place the ironing table on a sturdy, non-slippery, smooth surface.  

USAGE  OF THE APPLIANCE AND OPERATION  

1. Put the folded table on the ground in upright position.

2. Pull the spring lock handle so as to free the lock spindle from the lock box while holding the table on its nose with the other hand to incline it backward so that the legs get free from the ground. Thus, you can move the legs through the channel.
3. Using the lock handle, unfold the movable legs. After placing the bar in the channel for the desirable level of height adjustment, leave the lock handle free to fix the legs.

4. Using both of your hands, get the table in horizontal position. While doing this, do not lift the table up from the ground, but roll it down slowly towards the front with the two back legs stepping on the ground.

5. Be sure that the appliance does not have any electric connection.

6. Remove the cap of the water tank by turning in direction of counter-clockwise.

7. Fill tap water by using funnel and scaled glass which are available in the box.

      RECOMMENDATION: Ready hot tap water can be usable if available any. In this manner,  

      the appliance can be ready for ironing within a shorter period of time.

     WARNING: Usable water;

     Top water, Distilled or demineralised water. If the tap water is too hard, it can be mixable to               

      a good quality of pure water with the ratio1/2. A hundred percent pure water should not be 

     used.

8. After the completion of this procedure, close the cap of the water tank tightly. But not too tight!

9. Unwind the supply cable and the pedal cable wound on the short legs, located back of the control box and designed for winding cables on, and put the pedal on the ground and insert the plug in the socket.
10. Turn on the switch for steam boiler (1) and switch for iron (2) which are located on the control panel of the appliance.

11. Use the temperature setting knob (3) to adjust the ironing surface temperature to the desired value. Depending on your operation, the resistance engaged signal (4) light will go on and off to ensure the preset value of temperature.

12. To get the appliance ready for ironing; Wait until steam ready signal (6) lamp lights up.( This period is approximately 10 minutes.)

      WARNING: Do not open the cap of the water tank definitely after this stage.
      NOTE: The situation is considered to be normal if it lamps gets on and off during ironing.
13. You ought to adjust the thermostat knob of your iron for required temperature settings according to the varied fabrics.

       The following temperature setting table indicates the most appropriate temperature knob      

       positions for different sorts of fabrics.  

	TEMPERATURE SETTING TABLE

	Fabric Type
	Thermostat Knob Position 

	Synthetic garments, Acrylic, Silk, Polyamide, Acetate, Orlon, Nylon, Polyester, Viscose, Artificial Textile.
	

	Wool, Rayon.
	

	Cotton
	

	Linen
	


14. Unite the two parts of spring antenna and install the spring antenna into the steam boiler. Hook the cable through the hole of the spring antenna. 

15. Steam controlling button of the iron should be pressed a few times, keeping away from the ironing table that can prevent your garments from wetness due to the unexpected dripping water from iron.

16. So long as the vapor is shooted away during the ironing operation, press on the pedal for a sufficient period of time to suck the vapor.

           Now you may start ironing with pleasure. Any kind of fabric can be professionally ironed easily,             

           within a very short period thanks to the intense and continual steam producing features of the 

           appliance. You may place the iron on the iron resting base of the appliance. 

TO REFILL WATER DURING IRONING IF REQUIRED
· When the water is completely consumed during ironing, switch for steam boiler (1) lamp will go off and  no water (7) lamp will go on. 
· Steam output stops.
· Needle of the manometer will fall to zero position.

1. Unplug the appliance.  

2. Switch (1) and (2) on the control panel to OFF position. 
3. Do not open the cap of the water tank suddenly as some steam could be left in the steam boiler. Turn the cap of the water tank gradually and stop at the steam releasing point and await until all the steam is released.   

4. After completion of this process, open the cap, fill the required portion of water by using funnel and scaled glass. 
              WARNING: At this stage, while performing the water filling process, fill the water carefully 

              little by little, otherwise hot water may leap on you as the steam boiler could still be hot. 

              After a while, the temperature of the boiler will be at a normal level and then you may 

              continue to the normal process of water filling.   
5. Check for the excess water in the water tank by means of scaled level control tube. 

6. Plug in the appliance. 

7. Switch (1) and (2) on the control panel to ON position. 
You may continue from the stage you left ironing soon after the steam ready (6) lamp goes on.  

AFTER THE OPERATION 

                  When you complete the ironing operation, firstly;

1. Switch (1) (2) and (3) on the control panel to OFF position.  

2. Then unplug the appliance and let it cool down for a certain period of time.

3. After the ironing surface cooled down enough, you can fold the appliance and put it away in an appropriate place if necessary. 

4. Open the valve underneath the boiler, with the help of handle which is placed in front of boiler, and empty the useless water left in the boiler.
5. Folding up the appliance needs just the reverse of the operations what you did while unfolding it. Namely, you ought to follow in sequence:

I. Rewind the cables and steam hose on the short legs at the rear of the control box and put the steam iron on the iron resting base.

II. In order to be able to fix the iron;  stretch the elastic belt and interlock the hook-eye of the elastic belt on the metal frame as you see on top of steam boiler.

III. Incline the table backward such that it will press on the short legs at the rear of the control box and the rear legs and put it to upright position. 

IV. Pull the lock handle to free the movable legs out of the distance channel that is underneath the ironing surface and incline the table slightly backward such that it will press only on the short legs at the rear of the control box.

V. Fold the legs until the lock spindle levels with the lock box such that it will remain locked when the table is folded, and leave the lock handle free.

VI. Store the table away in a safe way that it would not overturn.

   PERIODIC CARE
           Weekly;

1. Unplug the appliance. 

2. Fill in tap water half the water tank and mix well. 

3. Open the valve, where is underneath the water tank, so that the water is poured down. Repeat this procedure at twice.  

CLEANING
1. Clean the appliance with a moist cloth.

2. Prevent the steam exit holes of the iron soleplate from being stopped up by remmant of lime, which is originating from water, by carefully cleaning it with a metal spit. The life of the iron will be longer if its soleplate will be cleaned with a thick moist cotton cloth when it is tepid. Difficult unremovable remmant can be formed with time if the holes of iron soleplate is not cleaned regularly. 

WARNING: Do not clean the iron soleplate under water or by plunging into water by no means.

           ATTENTİON !: Do not use any kind of materials like metal cleaning tools, detergents, lime remover 

           chemicals and abrasive materials for the cleaning of the iron soleplate.
	PROBLEMS AND SOLUTIONS

	Problem
	Reason
	Solution

	· ON/OFF switches on the front panel does not light
	· No electricity.

· Not connected to electricity.

· Broken socket.
	· Insert plug to the socket properly

· Check the socket

	· Steam output is insufficient or none.
	· Water tank is empty

· ON/OFF switch of boiler is OFF.

· Steam pressure level is low.

· Hose is bended.

· Electric disconnection.  In this case, no sound comes from the valve inside the appliance body in spite of pressing the steam control button of the iron.
	· Fill the tank

· Turn ON the switch with steam symbol and wait until “steam” lamp lights up.

· Wait until steam pressure reaches more than 1.5 bars.

· Check the hose and make it smooth.

· Contact Silter Authorized Service.

	· Boiling water pop when I fill the water.
	· Water is refilled while the boiler is still hot.
	· Wait a couple of minutes. When the boiler cools down , you may continue to refill.   

	· There is enough water in the tank but “No Water” lamp is still lit.
	· Electricity fault.
	· Disconnect the appliance from the electricity. Contact Silter Authorized Service.

	· Cap of the water tank is closed well but steam is still leaking.
	· Rubber o-ring damaged.

· Mechanical fault.
	· Replace the rubber o-ring inside the  cap.

· Disconnect the appliance from the electricity. Contact Silter Authorized Service.

	· The needle of the manometer displays the pressure more than 5 bars.
	· Electric or mechanical fault.
	· Disconnect the appliance from the electricity. Contact Silter Authorized Service.

	· “Steam” lamp turns on and off during operation.
	· It is not a problem. 
	· You can continue to work.

	· Dripping water through the iron.
	· Tank is overfilled

· The lime and sediment ratio of water in the tank raised.
	· Empty the extra water:

· Fill in the water half the boiler, rinse with water and empty
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