ВЫБОР СТРОЧКИ ДЛЯ РЕДАКТИРОВАНИЯ
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1. Установите устройство для вышивания на машину (см. стр. 5-5).
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2.  Для того, чтобы вызвать экран, изображенный на рисунке слева, нажмите клавишу
Клавиша
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Тип строчки
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Точечная строчка
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Алфавит в цветами
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Строчка, сохраненная в памяти машины
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Знаковая строчка
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Обрамляющая строчка
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Строчка с картриджа (картриджи продаются отдельно)
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Строчка с дискеты

Примечание

Если Ваша машина не укомплектована встроенным дисководом, Вы можете обратиться к авторизованному дилеру, который установит дисковод и сделает необходимые усовершенствования Вашей машины.
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Метод выбора строчки, не содержащей букв или знаков, идентичен методу выбора строчки для вышивания.
1.  Выберите тип строчки, который Вы хотите использовать.
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2.  Нажмите на клавишу выбранной строчки.
*   Более полную информацию о методе выбора строчки, Вы можете найти на стр. 5-8.
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3. строчка высветится в верхней части экрана.
4. После того, как Вы выбрали строчку, нажмите клавишу “SET”.
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5. На экране появится окно редактирования (см. рисунок слева)
*   Более полную информацию о редактировании строчки Вы можете найти на стр. 6-8.
1. Строчка, выбранная для редактирования, выделена красной рамкой.  
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Selecting Character Patterns
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1.  Press
to select character patterns.
When you select character patterns from the embroidery edit screen, you can edit the appearance of the pattern at the same time.
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2. Select the font.
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3. Enter the letters (Example: А В С D)
*   See page 5-11 for more information about selecting character;
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Press
to check the pattern when the selected characte
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4. Press array! to select the appearance of the pattern.
are too small to see clearly.
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5. The screen at left displays.
Select the appearance you want to use (Example:
to change the de-
Щ to make the arc flatter, to make the arc rounder.
After selecting the curve, use
and
gree of the arc.
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Press
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6.   Press
to return to the original screen.
*   Press
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8. The embroidery edit screen will appear. See page 6-8 for more information about editing the patterns.
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0 Shows the size of the entire combined pat​tern.
Shows the size of the pattern currently se​lected.
If the pattern location has been moved, this area shows the distance from the center of the frame.
4) Shows the degree of ro​tation for the pattern. Shows the color cur​rently selected , and number of colors in the pattern.
Note —————————— If a key display is light gray, you can not use that func​tion with the selected pat​tern.
Key Functions
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6-8
Embroidery Edit Functions
Moving the Pattern
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Press
1
Press "i"1 to return the pattern to its original position.
to move the pattern in the position shown on the key.
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Shows how far from the original position the pattern is now.
Rotating the Pattern
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1.  Press
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2. Press
to rotate the pattern 90 deg. to the left.
Press
to rotate the pattern 90 deg. to the right.
Press
to rotate the pattern 1 deg. to the left.
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Press
to rotate the pattern 1 deg. to the right.
presc hSSS'l *0 retum the pattern to its original position.
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Shows the degree of the pattern's rotation
3. After changing the pattern, press
� EMBED Word.Picture.8  ���
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